## ModelicaAdditions.HeatFlow1D.Interfaces

Connectors and partial models for 1D heat flow

## ModelicaAdditions.HeatFlow1D.Interfaces.Surface_b

1D Heat flow connector (non-filled icon)

### Modelica definition

    connector Surface_b "1D Heat flow connector (non-filled icon)"
      SI.Temperature T "Absolute temperature";
      flow SI.HeatFlowRate q "Heat flowing into element";

    end Surface_b;

## ModelicaAdditions.HeatFlow1D.Interfaces.Surface_a

1D Heat flow connector (filled icon)

### Modelica definition

    connector Surface_a "1D Heat flow connector (filled icon)"
      SI.Temperature T "Absolute temperature";
      flow SI.HeatFlowRate q "Heat flowing into element";

    end Surface_a;

## ModelicaAdditions.HeatFlow1D.Interfaces.AbsoluteSensor

Device to measure a single connector variable

### Information

This is the superclass of a 1D component with one surface and one output signal in order to measure a heat flow quantity in the surface and to provide the measured signal as output signal for further processing with the Modelica.Blocks blocks.

Release Notes:

- June 15, 2000 by Martin Otter:
  Realized.

### Modelica definition

    partial model AbsoluteSensor
      "Device to measure a single connector variable"

      extends Modelica.Icons.TranslationalSensor;

      Surface_a surface_a;
      Modelica.Blocks.Interfaces.OutPort outPort(final n=1);
    end AbsoluteSensor;

## ModelicaAdditions.HeatFlow1D.Interfaces.RelativeSensor

Device to measure a single relative variable between two surfaces

### Information

This is a superclass for 1D components with two surfaces and one output signal in order to measure relative quantities between the two surfaces and to provide the measured signal as output signal for further processing with the Modelica.Blocks blocks.

Release Notes:

- June 15, 2000 by Martin Otter:
  Realized.

### Modelica definition

    partial model RelativeSensor
      "Device to measure a single relative variable between two surfaces"

      extends Modelica.Icons.TranslationalSensor;

      Surface_a surface_a;
      Surface_b surface_b;
      Modelica.Blocks.Interfaces.OutPort outPort(final n=1);
    end RelativeSensor;