Node:GDB/MI Output Syntax, Next:GDB/MI Simple Examples, Previous:GDB/MI Input Syntax, Up:GDB/MI Command Syntax

#### GDB/MI Output Syntax

The output from GDB/MI consists of zero or more out-of-band records followed, optionally, by a single result record. This result record is for the most recent command. The sequence of output records is terminated by `(gdb)`.

If an input command was prefixed with a ``token`` then the corresponding output for that command will also be prefixed by that same token.

``output`==>`
  `(` out-of-band-record`)* [` result-record`] "(gdb)"` nl``
``result-record`==>`
  `[` token`] "^"` result-class`( ","` result`)*` nl``
``out-of-band-record`==>`
  ``async-record`|` stream-record``
``async-record`==>`
  ``exec-async-output`|` status-async-output`|` notify-async-output``
``exec-async-output`==>`
  `[` token`] "*"` async-output``
``status-async-output`==>`
  `[` token`] "+"` async-output``
``notify-async-output`==>`
  `[` token`] "="` async-output``
``async-output`==>`
  ``async-class`( ","` result`)*` nl``
``result-class`==>`
  `"done" | "running" | "connected" | "error" | "exit"`
``async-class`==>`
  `"stopped" |` others`` (where others will be added depending on the needs--this is still in development).
``result`==>`
  `` variable`"="` value``
``variable`==>`
  `` string``
``value`==>`
  `` const`|` tuple`|` list``
``const`==>`
  ``c-string``
``tuple`==>`
  `"{}" | "{"` result`( ","` result`)* "}"`
``list`==>`
  `"[]" | "["` value`( ","` value`)* "]" | "["` result`( ","` result`)* "]"`
``stream-record`==>`
  ``console-stream-output`|` target-stream-output`|` log-stream-output``
``console-stream-output`==>`
  `"~"` c-string``
``target-stream-output`==>`
  `"@"` c-string``
``log-stream-output`==>`
  `"&"` c-string``
``nl`==>`
  `CR | CR-LF`
``token`==>`
  any sequence of digits.

Notes:

- All output sequences end in a single line containing a period.
- The ``token`` is from the corresponding request. If an execution command is interrupted by the `-exec-interrupt` command, the token associated with the `*stopped` message is the one of the original execution command, not the one of the interrupt command.
- status-async-output contains on-going status information about the progress of a slow operation. It can be discarded. All status output is prefixed by `+`.
- exec-async-output contains asynchronous state change on the target (stopped, started, disappeared). All async output is prefixed by `*`.
- notify-async-output contains supplementary information that the client should handle (e.g., a new breakpoint information). All notify output is prefixed by `=`.
- console-stream-output is output that should be displayed as is in the console. It is the textual response to a CLI command. All the console output is prefixed by `~`.
- target-stream-output is the output produced by the target program. All the target output is prefixed by `@`.
- log-stream-output is output text coming from GDB's internals, for instance messages that should be displayed as part of an error log. All the log output is prefixed by `&`.
- New GDB/MI commands should only output lists containing values.

See GDB/MI Stream Records, for more details about the various output records.